Here are the three alignment specs we have for Mustangs:


Street 
Front camber -1.03 degrees on both sides (Performance and Handling Pack)
Front camber -.72 degrees on both sides (non-Performance and Handling Pack)
Caster +7.0 degrees on both sides
Front toe +0.01 degrees per side total toe of +0.02 degrees, this is toe in
Rear camber -1.5 degrees on both sides
Rear toe +0.115 degrees per side, total toe of +0.23 degrees, this is toe in


DRAG
This is drag race only.
Front camber -0.75 degrees, must be even on both sides.
Caster +7.0 (+/- .25 degrees), must be even on both sides.
Front toe +0.01 per side, total toe +0.02. This toe in.
Rear camber -0.5 degrees (+/- .25 degrees), must be even on both sides.
Rear toe +0.12 degree, must be even on both sides. This toe in.


Track
Typical track/autocross alignment settings(not street use);
Front camber -3.0 degrees on both sides
Caster +7.0 degrees on both sides
Front toe +0.01 degrees per side total toe of +0.02 degrees, this is toe in
Rear camber -1.6 to -1.7 degrees on both sides
Rear toe +0.12 degrees per side, total toe of +0.24 degrees, this is toe in

